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Channel Partner Price List
1. Smart Cards/Proximity Cards
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	· Thick proximity clamshell card 125 KHz 4100 chip – Price: Rs. 6.25

· Thin proximity ISO card 125 KHz 4100 chip – Price: Rs. 8.50/-

· Proximity13.56 MHz (1K MF)– Price: Rs. 9.75/-

· MiFare 1K S50 (Philips,NXP) card 13.56 MHz – Price: Rs. 22/-

· MiFare 4K S70 (Philips,NXP) card 13.56 MHz – Price: Rs. 39.00/-

· Mifare Desi Fire 4K card – Price :Rs.62.00/-

(Free Delivery for more than 2000 qty by road)



	Also available Contact less Smart Cards List



	MIFARE 1 S50 – PHILIPS                EM4135 (13.56M)      ATA5590 UHP – ATMEL


	MIFARE 1 S70 – PHILIPS                EM4222 UHF             SR-176 – ST


	MIFARE 1 Ultra light – PHILIPS      EM4223 UHF            T5557 – ATMEL


	I-Code1, 2, SLI * - PHILIPS              EM4422 UHF             88RF256-12 – ATMEL


	HITAG1, 2, S * - PHILIPS                 EM4100                      LEGIC MIN256


	MIFARE D40 – PHILIPS                   EM4102                      INSIDE – 2K *


	I-Code UID – PHILIPS                       EM4450                      INSIDE – 16K *


	I-Code EPC 13.56M – PHILIPS         EM4035 (13.56M)      SLE66R35 – SEIMENS



2. Accessories
	Z-L-Bracket
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SP:Rs.850/-

	U-Bracket 
[image: image2.png]



SP:700/-

	EM Lock
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SP:2000/-

(Auto Feedback & Magnetic Control)
          
	Bolt Lock
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Rs.1500/-                                SP:Rs.2500/-

	Electric Strike Lock 
[image: image5.png]



SP:Rs.1850/-

	EM Lock with LED 
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SP:Rs.1800/-


3. CCTV
	Titania 804
	Descriptions
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SP:Rs.1800/-
	· 1/3” color CCD,

· 420TVL,10M,

· Indoor plastic dome camera,

· 3.6mm lens



	Titania 668111
	Descriptions

	[image: image28.png]



SP:Rs.3000/-
	· 1/3”Sony chipset

· 420TVL,Sony DSP,

· 15M,20LED,

· 6mm lens

· Metal housing,Glass

· IR Camera



	Titania 66811
	Descriptions
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SP:Rs.3000/-
	· 1/3”Sony chipset,

· 420TVL,Sony DSP,

· 15M,23LED,

· 3.6mm lens, with cut-proof bracket

· IR Camera

	Titania 668
	Descriptions
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SP:Rs.3000/-
	· 1/3”Sony chipset,
· Sony DSP,
· 420TVL,15M,
· 6mm lens
· 24LED,with bracket
· IR Waterproof Camera
· Metal Housing

	Titania 2004SN
	Descriptions
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SP:Rs.4000/-
	· 1/3”Sony super HAD CCD

· 420TVL,35m,

· 24LED,with  bracket

· 3.6mm lens
· IR Waterproof Camera

· Metal housing



	Titania 2006SN
	Descriptions
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SP:Rs.3800/-
	· 1/3”Sony super HAD CCD+Sony DSP,

· 420TVL,10m,

· 12LED,plastic dome,

· 3.6mm lens

· IR Camera


	Titania 1420
	Descriptions
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SP:Rs.5250/-
	· 1/3”Sony super HADIICCD,

· 420TVL,50m,

· 32LED,plastic dome,

· 12mm lens

· IR Water Proof Camera


4. DVR

	Titania2004
	Descriptions
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SP:Rs.8000/-
	· 4CH-M-JPEG Standalone DVR without VGA



	Titania2004With VGA
	Descriptions

	[image: image35.jpg]¢




SP:Rs.9000/-
	· 4CH-M-JPEG Standalone DVR with VGA



	Titania SD04
	Descriptions
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SP:Rs.15000/-

	· H.264-4 CH Standalone DVR with  1 Channel Audio output



	Titania SD08
	Descriptions

	[image: image37.jpg]



SP:Rs.20000/-
	· H.264-8 CH Standalone DVR with  1 Channel Audio output
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Titania S16 without Audio
	Descriptions

	SP:Rs.30000/-
	· H.264-16 CH Standalone DVR without Audio output



	Titania S16 with Audio
	Descriptions
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SP:Rs.30000/-
	· H.264-16 CH Standalone DVR with  4 Channel Audio output




5. Fingerprint Based Time & Attendance

	eSSL H3006
	Fingerprint based Time & Attendance System
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SP:Rs.8000/-
	Specifications:

·  32 Bit high speed embedded processor

· 1500FP Templates & 50000 Transaction

· 500 DPI Optical Sensor

· Communication: USB
· Inbuilt Battery Backup

· T&A Software with Vistor Management- eTimeTrackLite with MSAcess free

· Also available MS-SQL and Oracle version

	
	

	eSSL-E9999
	Fingerprint based Time & Attendance System
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Sp:Rs.15000/-

	Specifications:

·  32 Bit high speed embedded processor

· 1500FP Templates & 50000 Transaction

· 500 DPI Optical Sensor

· Communication: TCP/IP,RS232/485,USB
· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free

· Also available MS-SQL and Oracle version
Optional : 

· Proximity Card Reader : Rs.1000/-extra

	FTA6161T
	Fingerprint based Time & Attendance System
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SP : Rs.18000/-

	Specifications:

·  32 Bit high speed embedded processor
· 3.0” Digital color TFT 

· 3000FP Templates & 1,00,000 Transaction

· 500 DPI Optical Sensor

· Communication: TCP/IP,RS232/485
· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free

· Also available MS-SQL and Oracle version
Optional : 

· Proximity Card Reader : Rs.1000/-extra

	FTA6030
	Fingerprint based Time & Attendance System
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SP:Rs.20000/-
	Specifications:

·  32 Bit high speed embedded processor
· 3.0” Digital color TFT 

· 3000FP Templates & 1,00,000  Transaction

· 500 DPI Optical Sensor

· Communication: TCP/IP,RS232/485/USB
· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free

· Also available MS-SQL and Oracle version
Optional : 

· Proximity Card Reader : Rs.1000/-extra

· Battery Back-up : 1000/-extra

	X990
	Fingerprint based T & A System(Optional Access Control)
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SP:Rs.22000/-

	Specifications:

·  32 Bit high speed embedded processor

· 1500FP Templates & 50000 Transaction

· 500 DPI Optical Sensor

· Communication: TCP/IP,RS232/485/USB
· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free

· Also available MS-SQL and Oracle version
Optional : 
· Proximity Card Reader : Rs.1000/-extra

· Smart Card Reader : Rs.2000/-extra

· Internal Battery Back-up(4000MAMP): Rs.1500/-
· Wifi : Rs.2000/-extra

· GPRS : Rs.6000/-extra
· Access Control: Rs.500/-extra
· Push Data Technology :Rs.2000/- extra
· Secugen Sensor optional @Rs.4000 extra


	FTA S-20
	Fingerprint based Time & Attendance System
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SP:Rs.24000/-

	Specifications:
· Q-Touch Keypad
· 3.0” Digital color TFT 

· 500 DPI Optical Sensor

· Communication: TCP/IP,RS232/485/USB

· 32 Bit High speed embedded processor
· 3000FP Templates & 1,00,000  Transaction

· Card Reader: Inbuilt Proximity Card reader
· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free

· Also available MS-SQL and Oracle version
Optional : 

· Smart Card Reader : Rs.1000/-extra
· HID(iProx) Card Reader : Rs.4000/-extra

	FTA1818
	Fingerprint based Time & Attendance System
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SP:Rs.24000/-
	Specifications:

·  32 Bit high speed embedded processor

· 1500FP Templates & 50000 Transaction

· 500 DPI Optical Sensor

· Communication: TCP/IP,RS232/485/USB
· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free

· Also available MS-SQL and Oracle version
Optional :

· Mifare card reader : Rs.1000/-

· HID(iProx) card reader : Rs.4000/-


	
	

	FTA5454
	Fingerprint based Time & Attendance System
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SP:Rs.24000/-
	Specifications:

·  32 Bit high speed embedded processor

· 3500FP Templates & 50000 Transaction

· 500 DPI Optical Sensor

· Communication: TCP/IP,RS232/485/USB
· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free

· Also available MS-SQL and Oracle version
Optional :

· Mifare card reader : Rs.1000/-                 


6. Fingerprint Based Time & Attendance/Access Control System
	eSSLF7A2
	Fingerprint based T&A cum Access Control
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SP:Rs.17000/-
	Specifications:

·  32 Bit high speed embedded processor

· 500FP Templates & 30000 Transaction

· 500 DPI Optical Sensor

· Communication: TCP/IP,RS232/485
· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free

· Also available MS-SQL and Oracle version
Optional :

· PSU : Rs.250/-extra(12V 1Amp)

· PSU:Rs300/- extra(12V 2 Amp)      

	FBAC9090/2727
	Fingerprint based T&A cum Access Control
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SP:Rs.18000/-
	Specifications:

·  32 Bit high speed embedded processor

· 500FP Templates & 30000 Transaction

· 500 DPI Optical Sensor

· Communication: TCP/IP,RS232/485
· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free

· Also available MS-SQL and Oracle version
Optional :
· PSU : Rs.250/-extra(12V 1Amp)
· PSU:Rs300/- extra(12V 2 Amp)

	FBAC603
	Fingerprint& Card based T&A cum Access Control
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   SP:Rs.18000/-
	Specifications:
· Size: 180(L)*82(W)*55(H)mm

· User capacity:1500;Transaction Storage:50000

· Inbuilt proximity card reader

· Electric lock control: Directness relay output12VDC

· Communications:RS232/485,TCP/IP/USB

· Sensor: Optical sensor 500 DPI

· Support external 26 bit Weigand reader for exit

· Weigand out to connect 3rd party Controller

· Support external Fingerprint reader Sr100

· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free

· Also available MS-SQL and Oracle version
Optional:
· Mifare Card  reader : Rs.1000/-extra

· HID card reader : Rs.4000/-extra

· PSU : Rs.250/-extra(12V 1Amp)
· PSU:Rs300/- extra(12V 2 Amp)


	FBAC-9
	Fingerprint& Card based T&A cum Access Control
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SP:Rs.18000/-
	Specifications:
· Size: 180(L)*82(W)*55(H)mm

· User capacity:1500;Transaction Storage:50000

· Inbuilt proximity card reader

· Electric lock control: Directness relay opt12VDC

· Communications:RS232/485,TCP/IP/USB

· Sensor: Optical sensor 500 DPI

· Support external 26 bit Weigand reader for exit

· Weigand out to connect 3rd party Controller

· Support external Fingerprint reader Sr100

· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free

· Also available MS-SQL and Oracle version
Optional:
· Mifare Card  reader : Rs.1000/-extra

· HID card reader : Rs.4000/-extra

· PSU : Rs.250/-extra(12V 1Amp)
· PSU:Rs300/- extra(12V 2 Amp)   

	702E With SR100
	Fingerprint& Card based T&A cum Access Control
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SP:Rs.22000/-
	Specifications:
· Size: 180(L)*82(W)*55(H)mm

· User capacity:1500;Transaction Storage:50000

· Inbuilt proximity card reader

· Electric lock control: Directness relay opt12VDC

· Communications:RS232/485,TCP/IP/USB

· Sensor: Optical sensor 500 DPI

· Support external biometric exit reader 

· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free

· Also available MS-SQL and Oracle version
Optional:
· Mifare Card  reader : Rs.1000/-extra

· HID card reader : Rs.4000/-extra

· SR100 With Proximity card reader : Rs.1000/-extra/-
· PSU : Rs.250/-extra(12V 1Amp)
· PSU:Rs300/- extra(12V 2 Amp)

	
	

	iClock990
	Standalone IP based TFT-Fingerprint T&A cum Access Control Terminal
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SP:Rs.30000/-
	Specifications:
· 32 Bit High speed embedded processor

· User Capacity: 10,000 FP

· Transaction Storage: 1,50,000 Transaction
· Card Reader: Inbuilt Proximity Card reader

· Color TFT screen,VGA camera, battery back-up

· Communications:TCP/IP,RS232/485, and USB

· Support external 26 bit wiegand reader for exit

· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free

· Also available MS-SQL and Oracle version
Optional:
· Camera  :Rs 1500/- extra

· Internal Battery Back-up(4000MAMP): Rs.1500/-
· Mifare card reader : Rs.1000/- extra

· HID card reader : Rs.4000/- extra

· Wifi : Rs.2000/- extra

· GPRS : Rs.6000/-extra
· Secugen sensor optional @Rs.4000

	S900
	Fingerprint based T&A Cum Access control(Secugen Sensor)
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SP:Rs.30000/-
	Specifications:
· Rugged Scratch-resistant Secugen sensor

· User Capacity:1500,Transaction Storage :50000

· Card Reader: Inbuilt EM RFID (Proximity) Card reader

· Colour TFT Screen

· Communication: TCP/IP,  RS 232/485 ,USB

· Supports external 26 bit Wiegand reader for exit
· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free

· Also available MS-SQL and Oracle version




7. Face Recognition Systems
	iFace201
	Face+Card based Time& Attendance/Access Control 
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SP:Rs.30000/-
	Specifications:

· User  capacity : 1500 face & 10000 cards

· Transaction capacity : 100000 logs

· 32 bit high speed embedded processor

· High definition infrared camera

· Sensor : 500 DPI optical sensor

· Communications: TCP/IP,  RS 232/485 ,USB
· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free

· Also available MS-SQL and Oracle version



	
	

	iFace202
	Face+ Finger+card based Time& Attendance/Access Control
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SP:Rs.30000/-
	Specifications:
· User  capacity : 700 face (1:G first group 100 faces and subsequent groups 50 faces each), 10000 cards &3000 FP.
· Transaction capacity : 100000 logs

· Ultra high speed 32 bit  processor

· High definition infrared camera

· Sensor : 500 DPI optical sensor

· Communications: TCP/IP,  RS 232/485 ,USB
· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free

· Also available MS-SQL and Oracle version
Optional : 
· Proximity card reader ;Rs.1000/-extra

· Wifi : Rs.2000/-extra

· GPRS : Rs.6000/-extra
· Inbuilt battery backup Rs1500/- extra



	iFace302
	Face+ biometric based Time& Attendance/Access Control
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SP:Rs.30000/-

	Specifications:

· User  capacity : 700 face (1:G first group 100 faces and subsequent groups 50 faces each), 10000 cards &3000 FP.
· Transaction capacity : 100000 logs

· 32 bit high speed embedded processor

· High definition infrared camera

· Sensor : 500 DPI optical sensor

· Communications: TCP/IP,  RS 232/485 ,USB
· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free

· Also available MS-SQL and Oracle version

Optional : 

· Proximity card reader ; Rs.1000/-extra

· Wifi : Rs.2000/-extra

· GPRS : Rs.6000/-extra

· Inbuilt battery backup Rs1500/- extra


8. RFID Card Based Time & Attendance/Access Control System

	eSSL 2007 (K200)
	Proximity card based Time & Attendance system
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SP:Rs.12000/-
	Specifications:

· 32 Bit High speed embedded processor

· 30,000 card capacity & 30000 transaction storage

· Card Reader: Inbuilt EM RFID(Proximity) Card reader

· Communication: TCP/IP

· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free

· Also available MS-SQL and Oracle version
Optional : 

· USB : Rs.500/-extra

	Note: All card system attendance models (eSSL 7002, eSSL7020, eSSL2070) cost Rs 3,400/- with USB Rs .500/- extra


	SC 405
	Proximity card based Access Control & Attendance system
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SP:Rs.13000/-
 
	Specifications:

· 32 Bit High speed embedded processor
· Card Capacity: 10,000/- Storage capacity: 50,000/-

· Card Reader: Inbuilt EM RFID (Proximity) Card reader

· Supports external 26 bit Wiegand reader for exit
· Communication: TCP/IP and USB Pen drive

· T&A Software with Vistor Management- eTimeTrackLite with MSAccess free
· Also available MS-SQL and Oracle version
Optional:
· Smart card @ Rs. 1000/- extra

· PSU : Rs.250/-extra(12V 1Amp)
· PSU:Rs300/- extra(12V 2 Amp)


	
SP:Rs.2200/-
	Specifications:

· Dimension: 43mm(W) X 80mm(L) X 13mm(T) 
· Wgh: 61g Power: DC 9~12V, current: 30 –80 m A 
· Output: Weigand 26 Bit. 
· Working environment: -20°C~60°C,relative humidity: 5%--98%; 

	
	

	KR100 E
	Proximity Card reader / Mifare Smart card reader
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SP:Rs.2200/-
	Specifications:
· Dimension: 116*75*16 mm (L*W*T)

· Card Frequency: 125 KHz

· Proximity Range: >=5 cm

· Data Mode: Wiegand 26 bits

· Communication Distance: 100 meters

· LED indicator: Red, Green

· Speed: <= 0.2 sec


	
	

	No Touch 
	Exit Sensor

	
SP:Rs.1500/-
	Specifications:
· (115mm x 70mm x 33.5mm)

· Detection Range: Up to 4" (10cm)

· Voltage: 12VDC

· Uses IR technology to detect a wave of the hand and trigger a relay output

· LED indicator lights



9. Video Door Phone
	eSSL-278C-5  
	Standalone Colour Video door Phone

	SP:Rs.13000/-


	Specifications:

· Colour 7 inch TFT-LCD Screen

· Hands Free, Visitor Calling, Video Intercom, and monitor.

· With Warning Function.

· AV Output, CCD camera with LED lights.
· Four wire connection


Terms and Conditions:

Payment 100% upfront.

The prices are exclusive of taxes and freight charges.

Materials once sold cannot be taken back.

Warranty: 12 Months from invoice date excluding physical damage burnt Items etc.

Note: Warranty does not include power supply adaptor, SMPS, UPS, Cards, Exit readers and prism damages.

Note: Prices can change without any prior notice.
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